
Slater Project - Handwork
BID PACKET

August 5, 2026

*Project Funded by a USDA*

Project Summary
[bookmark: _Toc356296569]This fuel mitigation project is located in Happy Camp in Siskiyou County, California. The treatment will protect habitable structures in and around the community. The objective of this project is to provide immediate fuel mitigation to reduce fuel loading within the project area and to allow for prescribed fire lines to be created to facilitate underburning. Funding for this project is provided by the USDA Forest Service, State and Private Forestry through the California Association of Resource Conservation Districts.

Implementation must not begin before receiving the Notice to Proceed. 
[bookmark: _Toc356296571][bookmark: _Toc362767564][bookmark: _Toc82854507][bookmark: _Toc261602482][bookmark: _Toc356296572]Contractor’s Obligations
The Bidder must analyze and respond to all sections of this Bid Packet providing detailed information to allow the SVRCD to evaluate the bids. The Contractor, by submitting its bids, agrees that any costs incurred by the Contractor in responding to this Bid Packet, are to be borne by Contractor and may not be billed to the SVRCD.   

The Bidder must complete and submit all attachments in Appendix I, in the order listed. If the SVRCD has any confusion or difficulty in retrieving the required information from a Contractor’s bid, it may result in the disqualification of such bid.
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[bookmark: _Toc356296581][bookmark: _Toc261602484]
Bid Submission Requirements 
Submission of Bids: 
Contractor should mail, hand deliver, or email their bid to the address listed below by 2pm on September 4th, 2026. Hard or electronic bids will be accepted. 

Shasta Valley RCD 
215 Executive Ct., Suite B 
Yreka, CA 96097 
 
For hard copy bids, the envelope shall be plainly marked in the upper left-hand corner with the name and address of the bidder and shall bear the words “Bid for the Slater Project - Handwork”.

Electronic bids shall be sent to Dan Blessing, Project Manager at dblessing@svrcd.org. Please make the subject line “Bid for the Slater Project - Handwork” followed by your company’s name.
Critical Dates 
[bookmark: _Toc356296584]Pre-bid Site Visit
Contractors wishing to bid on this project may attend a pre-bid site visit scheduled on August 26th, 2026, at 9:30 am. Those interested will meet in Happy Camp at the corner of Highway 96 and Davis Road (Indian Creek Road). Representatives of the SVRCD and the City will be present to discuss the project. Please RSVP with the SVRCD if you plan on attending.
 
Dan Blessing, Project Manager  
Email: dblessing@svrcd.org	
Phone: 805-458-2684

Garrett Hickey, Project Manager
Email: ghickey@svrcd.org
Phone: 530-925-5430

Contract Dates
The Contractor shall not begin operations until the Notice to Proceed is issued. All work shall be completed by November 30th, 2026.
[bookmark: _Toc356296591][bookmark: _Toc261602487]Contractual Commitment of Bid
[bookmark: _Toc356296593]The contents of submitted bids will be considered obligations of the successful Contractor. No information should be submitted that is not intended to be incorporated into the bid and any contract, which may result from such bid. If there is any inconsistency between the terms herein and any of the contract documents, the terms in the contract documents shall prevail.
[bookmark: _Toc356296615][bookmark: _Toc261602491][bookmark: _Hlk45096748]Project Specifications
The contractor is expected to follow the project specifications, site plans, permit requirements, and all state, county, and city laws and standards for this project.

The objective of this project is to create a fuel break around private lands adjacent to Karuk properties to facilitate prescribed fire implementation on Tribal lands. Brush and dead vegetation will be removed by hand cutting to create the fuel break. Hand cut material will be piled. Dead and dying trees will also be removed.

Cutting Specifications: 
· Cut and remove live trees up to 8” DBH to achieve a 20-foot spacing 
· Cutters should abide by the following species preference in this order; Cedar, Maple, Madrone, Chinquapin, Live Oak, Bay (Pepperwood), Tan Oak, Ponderosa Pine, then Douglas Fir
· No cutting of Black Oak, White Oak, Yew, Sugar Pine, Dogwood, and Manzanita shall occur
· Cut all brush species except for manzanita 
· Cut all dead trees (snags) <20” DBH. Hazardous trees larger than 20” DBH that compromise safe working conditions may also be felled. Limb wood and boles less than 8” will be piled.
· Hardwoods, brush and conifers stump height no more than 4 inches from the ground as measured on the uphill side. Stumps shall not be cut at an acute angle
· Trees with the most desirable characteristics should be retained, i.e. healthy, full crowns, and disease free
· Any vegetation felled outside the project area will be brought back in for treatment
· All cut material up to 8" diameter must be piled. Preexisting ground fuels larger than 2" diameter and 2' length must also be cut and piled.
· Where slash is piled, keep piles no larger than 8 feet in diameter and a minimum 5'L x 5'W x 5'H. Slash shall be bucked into 6' lengths or less.
· No limbs and branches shall be left sticking out beyond the main body of the piles
· Piles shall be made at least 6 feet away from remaining trees and vegetation
· Cutter will limb all trees to shoulder height. All live limbs shall be completely severed from the remaining stump/bole of tree. Limbing will be performed in such a way that no damage to bole of limbed trees will occur
· On hardwoods such as tan oak, chinquapin, madrone, and maple where there are multiple stump sprouts, thin down to the healthiest largest three sprouts per clump
· Piles shall be covered with two 6' long pieces of 75/85 heavy duty wax paper. The covering should come down at least half the height of the pile and ensure that material is piled on top to prevent the craft paper from being blown off.  Paper should be placed at least ¾ of the height of the pile, wax up

Protection of Cultural Resources 
· A map of identified cultural resources will be provided. Contractor shall avoid disturbing these resources. Resources may be flagged with yellow-and-white striped flagging. All information shared with the contractor as part of this solicitation is confidential and will not be shared with those not associated with this contract.
· Discovery, by either the Contractor or the Shasta Valley Resource Conservation District, of cultural resources needing special protection shall be promptly reported to the Project Manager. Contractor shall immediately cease operations in the area. A perimeter of the protected resource shall be identified and avoided using yellow-and-white striped flagging.  

Protection of Sensitive Wildlife & Plant Species:
· Wildlife Limited Operating Periods will be in effect. No chainsaw operations will be performed during this time
· If wildlife is encountered during project activities, project work shall be paused to allow wildlife to leave area unharmed. Exclusion areas will be established around habitat elements such as active nests, dens, roosts, etc. Any such areas identified by Contractor must be reported to the Project Manager.
· In order to protect any species covered by the Migratory Bird Treaty Act (MBTA), fuels treatment between March 1 to August 31 must not occur until surveys are conducted by a biologist or a person with knowledge of, and ability to recognize, species protected by the MBTA and it is determined that there are no occupied nests within the proposed activity area. SVRCD staff or a contracted biologist will complete these surveys within 2 weeks prior to work beginning. If an MBTA species is located then no activities will occur within 100 feet of the nest during the breeding season (March 1- August 31).
· If Contractor discovers any sensitive wildlife or plant species, Contractor shall immediately contact the Project Manager and stop work within 100 feet of the sensitive species.


Protection of Aquatic & Riparian Habitat
· Intermittent and perennial water bodies will have buffers of 25 feet where no hand piles can be located. 
· At least 75% of the overstory canopy of native riparian vegetation will be retained within riparian buffers. Buffers will be flagged with blue & white striped flagging.

Boundaries: 
· The boundaries depicted on the project area map delineate the treatment unit. A georeferenced digital map will be provided to help Contractor identify unit boundaries using GPS assisted technology.
· A georeferenced map of riparian buffer zones will be provided. 
· Buffer zones for sensitive resources will be flagged with yellow & white striped flagging. A georeferenced map of these areas will also be provided. Sensitive resource areas will be treated by hand cutting but piles will be located outside of flagged areas.
· In areas where the digital map differs from on-the-ground flagging, any flagging present will prevail as the boundary.

Safety:
· Contractor shall be responsible for initiating, maintaining, and supervising all safety precautions and programs in connection with the performance of the work. 
· During the contract performance, Contractor shall protect the lives and health of workers performing the work and other persons who may be affected by the work and prevent damage to property adjacent to the project. 
· Contractor shall comply with all applicable laws, ordinances, rules, regulations, and orders of any public body having jurisdiction for the safety, of persons or property or to protect them from damage, injury, or loss; and shall erect and maintain all necessary safeguards for such safety and protection. 

Work progress: 
Contractor’s operations shall progress in a workmanlike and orderly manner to avoid accidentally leaving untreated areas, with workers regularly connecting treated areas. At the end of each workday, no “islands” of untreated areas shall be left within areas that have been treated.  
[bookmark: _Toc107722654][bookmark: _Ref108944804][bookmark: _Ref108946750][bookmark: _Ref108946754][bookmark: _Toc261602492][bookmark: _Toc261602493]Payment Schedule  
Invoices will be submitted to SVRCD on a monthly basis. The schedule is negotiable and will be refined during the contracting process.
Payments to the contractors shall be paid within thirty (30) days from receipt of the funds by the SVRCD from the funding agency, which can be as much as three months after invoice submittal for this particular grant. Every effort will be made to expedite payment to the contractor.
[bookmark: _Toc261602495]Additional Information
Site Location: This project is located on land within and around the community of Happy Camp. Land ownership includes Karuk Tribal Fee and Trust parcels. See maps in Appendix II for more information.
Subcontracting: Any subcontractors must be identified along with the defined work they will perform on the bid form provided. The SVRCD will not refuse a bid based on the use of subcontractors but does retain the right to refuse the subcontractors selected. Contractor shall remain solely responsible for all subcontracted work.

Insurance: The Contractor is required to provide SVRCD with proof of appropriate insurance listing the SVRCD as additionally insured.

General and Commercial Liability Insurance: 
The Contractor shall provide commercial general liability insurance of not less than $1,000,000 per occurrence for bodily injury and property damage liability combined for $2,000,000 in effect to the Contractor. 

Worker’s Compensation Insurance: 
The Contractor shall provide Worker’s Compensation Insurance with Waiver of Subrogation. Employer’s liability shall be not less than $1,000,000.00. 

Commercial Automobile Insurance on Owned, Hired, and/or Non-Owned vehicles: 
The Contractor shall provide Commercial Automobile Insurance on Owned, Hired, and/or Non-Owned vehicles of not less than $1,000,000.00 policy.
Limited Operational Periods: Work within may have periods where operations cannot be done due to species of concern or weather conditions. Current LOPs may be lifted with appropriate surveys completed to protocol.
Labor Compliance: Contractor agrees to be bound by all the provisions of the California State Labor code. 
Maps and Measurements: The maps are provided as Attachments. They are intended to show only the general size, shape, and location of the areas.  If the maps conflict with the field marking, the field markings shall govern.  Positions of features are approximate.  The units have been determined by Global Positioning Systems (GPS) and/or Geographic Information Systems (GIS).  If re-measurement of the acreage is desired by the contractor, notification shall be made upon written request.  Requests for re-measurement shall be made within 10 days after work has been completed on the unit.
Rework and Re-inspection after Rework: If contract specifications are not met as determined by Project Manager, payment may not be made until the problem has been corrected, unless the Project Manager determines that a reduction in pay in lieu of rework is acceptable.   
Safety: When Contractor’s operations are in progress adjacent to or on all roads. Contractor shall furnish, install, and maintain all temporary traffic controls which provide the road user with adequate warning of hazardous or potentially hazardous conditions associated with Contractor’s operations.  
Protection of Improvements and Survey Monuments: The Contractor shall avoid any damage to improvements such as, but not limited to: trails, telephone lines, pipelines, structures, roads, fences, gates, utility poles, power lines, pedestals, survey markers or monuments, and survey witness trees. The contractor will be required to repair or pay fair market value to replace any damaged improvements.

[bookmark: _Toc261602496]CERTIFICATION OF COMPLIANCE: Contractor shall certify compliance with specific fire precautionary measures included in the attached Fire Plan. The certification shall be made prior to commencement of work and shall be updated if at any time during performance the conditions change.









[bookmark: _Ref108944229]Attachments
Appendix I
· Bid Form Attachment No. 1: Contractor Information
· Bid Form Attachment No. 2: Proposed Subcontractors
· Bid Form Attachment No. 3: Bid Schedule
· Bid Form Attachment No. 4: Project Questionnaire
· Bid Form Attachment No. 5: Work Plan


[bookmark: _Hlk17468260]Appendix II
· Exhibit A: Project Map
· Exhibit B: Fire Plan







Appendix I



BID FORM ATTACHMENT NO. 1: Contractor Information

General Information:

	Company Name:
	

	

Company Address:
	

	

Contact Name:
	


	

Phone:
	

	

Fax:
	

	

Email:
	
	
Federal ID or SSN #:
	

	

Years in Business:
	
	
QAL (or equivalent) and LTO License #:
	




Bid Information
Bidder agrees to accept as full payment the following total base bid price:

           		_______ ___________________________   dollars
						(in words)

	       		________________________________________________________  
							(in numerals)
     
                     In the event of a discrepancy, amount in words shall prevail.

The bidder hereby acknowledges that the total base bid price is based solely on the bidder’s own estimate of costs and includes all applicable taxes, overheads, and profit.  

Contractor Signature__________________________________________________________________

Additional bid Information: Please provide detailed information as outlined in the bid schedule below.  Costs shown above should include all materials, labor, taxes, overheads, and profit, which must also be included in the following schedule.




BID FORM ATTACHMENT NO. 2: PROPOSED SUBCONTRACTORS 
 
The BIDDER should submit with the Bid Form a listing of names and business addresses of subcontracting firms or businesses that will be awarded subcontractors for portions of Work as described above.

The Subcontractor list shall be completed and should include the following information: 
1. Subcontractors, listing each subcontractor whose subcontract amount is more than 10 percent of the Contract price with whom the bidder, if awarded the Contract, will subcontract for performance. 
2. The categories of work those subcontractors will perform on the Contract. 

A bid will be considered non-responsive and will be rejected if the BIDDER does not correctly complete the Subcontract List contained herein and include this Proposed Subcontractor list with the Bid Form.
 
A. List of Subcontractors to be used 
	Subcontractor 
	 
	Work 
	 
	Dollar Amount 
	 
	% of Total 

	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 






BID FORM ATTACHMENT NO. 3: Bid Schedule


	Task No.
	DESCRIPTION (confirm based on plans and specifications)
	QTY.
	UNIT
	UNIT PRICE
	TOTAL

	1.0
	Handwork
	51
	ac
	 
	 

	[bookmark: _Hlk17717888]
	
	
	
	 
	 

	Total Bid Cost:
 
	 
	 
	 
	


Units: LS = Lump sum; ac = acre
[bookmark: _Hlk17730553]Pay items Description:
1.0 Handwork
The bid price for this item shall include all equipment, manpower, mobilization, insurance, and bonding to complete the work described in the specifications for handwork on this 51-acre area.




BID FORM ATTACHMENT NO. 4:  PROJECT QUESTIONNAIRE


Please initial _______ if contractor has direct previous experience fulfilling labor compliance requirements, including, but not limited to, wage determinations, submission of payroll records, etc.
	
If no direct previous experience, please list below who will assist in meeting this requirement. Please include contact information and experience.
________________________________________________________________________________



	



BID FORM ATTACHMENT NO. 5: WORK PLAN  
 
Please use the following space to describe in sufficient detail the work plan or methods you will employ to accomplish the project according to specifications. This will include a full description of how the project will meet the site requirements and prevent damage to infrastructure. You may attach a written response to this packet if needed.

	











Appendix II - Attachments


Attachment A

	Attached: Maps of Project Areas


Attachment B

Attached: Fire Plan
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